https://aliexpress.ru/item/32734965011.html?spm=a2g39.orderlist.0.0.4b534aa6TjNrHv&\_ga=2.231438559.1915488067.1633953984-919423421.1631208261

Advantage of coreless motor servo:

High reliability,   good stability,     strong adaptability,

 Low noise, small vibration, smooth operation, long life;

product description

**Size:**40\*20\*40(servo)

         64\*55.6\*20(Assembly the metal brackets size)

**Weight:**60g

**Wire length:**320mm

**Speed:** 0.13sec/60 degree at(5v)

              0.12sec/60 degree at(6v)

              0.11sec/60 degree at(7.4v)

**Torque:**29kg.cm.at(5v) -1.9A

32kg.cm.at(6v) -2.1A

                   35kg.cm.at(7.4v) -2.3A

**Voltage:** 5v-7.4v

**Dead Zoon setting:**2 Microseconds（RDS3235）

**Features:**

- Durable Metal Gear  
- Dual Ball Bearing  
- Programmable Digital Amplifier with Mosft Drive  
- Bottom Side Axial Mount Hole  
- Original factory product  
- Less Noise    
-Contains: Long Holder Aluminum & Short Holder Aluminum & Circle Holder-25T & Circle Holder -Orientation Angle:maximum 180 deg or 270 deg

-Mechanical Angle  :180 deg or 270 deg

(Plug/Output wheel/Radio control system compatible with Futaba JR Hitec)

**Package contains:**

1 pieces of RDS3235 Digital Metal Robotic Servo

1 pieces of long U metal brackets

1 pieces of short U metal brackets

1 pieces of metal servo arm 25T

1 pieces of metal servo arm driven

one set of screw(see the picture)

product pictures



